|  |  |
| --- | --- |
| Daytripper TX | |
| Parameter | **Value** |
| Dimensions  (Width-Height-Depth) | 28 x 36.5 x 19 mm  1.1 x 1.4 x 0.8 in |
| Weight | 20g  0.7oz |
| Max Detection Range | 120cm  4ft |
| Scan Rate  (Default) | 6Hz On Battery  30Hz Plugged In |
| Scan Rate  (User Configurable) | 1Hz - 30Hz |
| Battery Capacity | Rechargeable Li-Po  120mAh |
| Battery Life  (Default Configuration) | 50 Hours |
| Charging Time | 3 Hours |
| Connector | USB-C |
| Wireless Communication  Range with RX (Open Air) | 100m  330ft |

|  |  |
| --- | --- |
| Daytripper RX | |
| Parameter | **Value** |
| Dimensions  (Width-Length-Thickness) | 19 x 38 x 5 mm  0.8 x 1.5 x 0.2 in |
| Weight | 4g  0.14oz |
| Connector | USB-C |
| Actions | Minimise Windows (WIN+M)  Lock Computer (WIN+L)  Custom Action (ALT+PAUSE) |
| Compatible  Operating Systems | Anything that supports  USB keyboard!  Windows  macOS  Linux  Android  Raspberry Pi  etc |